INSTALLING NLD FCC ON DJI SMART REMOTE CONTROLLERS

** INTRODUCTION

These instructions are written for the DJI RC 2, but the same general
procedure can also be used with other DJI smart remote controllers.

NLD FCC does not require you to manually install any dependencies.
If additional components are required, NLD FCC will automatically acquire
and install them.

DJI has restricted APK installation on some consumer smart remote
controllers by removing the standard Android Package Installer.

To install NLD FCC, this restriction must first be removed by installing
the included Package Installer.

Once Package Installer has been installed, NLDFCC.apk can be installed
normally.



** INSTALLATION

1. Connect the RC 2 to your PC using USB and open its
   "Internal shared storage".

2. Copy the following extracted files to the RC 2 "Download" folder:
   * NLDFCC.apk
   * packageinstaller.apk

3. On the RC 2, swipe down from the top of the screen to open the system
   menu, then tap the Settings icon in the top-right corner.

4. Open:
   Storage -> Music & Audio -> Audio files
   This will open the Android file manager.

5. Tap the menu icon (three horizontal lines) in the top-left corner and
   select "Downloads".

6. Tap packageinstaller.apk and install it.

7. After installation, you will be returned to the "Music & Audio" screen.
   Tap "Audio files" again.

8. Open the menu, select "Downloads", and tap NLDFCC.apk.

9. If Android displays a warning about installing an unknown app, tap
   "Continue", then "Install".

10. When installation is complete, tap "Open".


** STARTING NLD FCC LATER

NLD FCC can be opened at any time from the notification area in the top
system bar, even after the NLD FCC application itself has been closed.
